\r – “Carriage Return”  
\n – “Line Feed”

CR has ASCII Value 13  
LF has ASCII value 10

CR points the printer to go back to exact start of the paper

LF would send printer to advance to next line.

Combination of them is still used for the specific purpose.